As used herein, "bone-facing side" refers to a side of an object, structure, instrument, or apparatus, such as an implant or instrument that is oriented toward or faces one or more bones of a patient when a device that includes the bone-facing side is in use. In one aspect, the bone-facing side may abut, touch, or contact a surface of a bone. In another aspect, the bone-facing side or parts of the bone-facing side may be close to, but not abut, touch, or contact a surface of the bone.

"Patient-matched" refers to a feature, aspect, attribute, characteristic, instrument, and/or device that is selected from a set of predetermined, predefined, precalculated, preconfigured, prearranged, and/or pre-fabricated structures, apparatuses, devices, instruments or devices to satisfactorily service a user based on a set of characteristics, such as size of an anatomical structure, deformity, fracture, laceration, opening, angles for certain landmarks, angles for a deformity, type of deformity, size of the bone, and the like. In certain embodiments, patient-matched is different from patient-specific.

"Patient-matched trajectory guide" refers to a trajectory guide that is patient-matched. In certain embodiments, a patient-specific trajectory guide is a trajectory guide that can be used on or in connection with a surgical procedure for a plurality of patient who share a common characteristic and/or attribute. A patient-matched trajectory guide serves as a guide for a trajectory to address a condition for the set of patients that satisfy one or more characteristics and/or attributes

"Patient-specific angle" refers to an angle that is patient-specific.

"Pin guide" refers to a pin, or wire such as a K-wire, that serves as a guide for a fastener (e.g., a cannulated fastener).

"Register" or "Registration" refers to an act of aligning, mating, contacting, engaging, or coupling one or more parts and/or surfaces of one object in relation to one or more parts and/or surfaces of another object. Registering and/or registration can include two parts or surfaces of different object abutting each other and/or coming into close proximity to each other. Often, the one or more parts and/or surfaces of one object include protrusions and/or depressions that are the inverse or mirror configuration of protrusions and/or depressions of one or more parts and/or surfaces of the other object.

"Remediation procedure" refers to any designed or performed for the purpose of remediating a condition of a patient and/or a condition of one or more parts of a body of a patient.

"Talar dome" refers to part of a talus bone. Specifically, the talar dome refers to the superior convex surface and/or area of the talus. The talar dome may also be referred to as a trochlea of the talus. The talar dome is part of the talus body.
